The initial organic material of topsoil will be stacked separately on a flat section 10m away from the cut, then the gold bearing gravels will be spread across in a separate area of the lease. After which it will be metal detected for course gold, then the pay dirt will be put through a dry blower. After the material has been treated the dirt will be moved to back fill the cut, after which the organic topsoil will be spread on top and leveled to original slope. This will be done to 2000 yards of material yearly if there are no mechanical breakdowns or natural disasters. As the material is alluvial and eluvial there is no hazards of sulfide contamination. Dry blowing dust will be controlled by only being operated in very low to no wind conditions. This process will be repeated and follow the gold bearing channel on the lease. Application 
